MULTISTANCE INTERNATIONAL
COMBAT SPORTS — TECH PACK TEMPLATE
Example base: Rash Guard + Fight Shorts — adapt rows for other combat styles (boxing, Muay Thai, wrestling, etc.)
This is a starting technical reference, not a final production specification. Fields shown as “[  ]” are for you to fill in or edit; standard values shown are Multistance's typical defaults and can be changed to match your requirements. Please complete this document and return it to your Multistance contact — our design team will use it to develop your product and formal quote. Once both parties confirm the final version, it will be attached as Exhibit A to your OEM Agreement.
1. Product Overview
	Field
	Buyer Specification

	Product / Style Name
	[  ]

	Discipline (MMA / BJJ / Muay Thai / Boxing)
	[  ]

	Components Included (Rash Guard / Fight Shorts)
	[  ]

	Rash Guard Sleeve Length (Short / Long)
	[  ]

	Fit (Compression)
	[  ]

	Target Market
	[  ]

	Order Quantity
	[  ]

	Target Delivery Date
	[  ]


2. Bill of Materials
“Multistance Standard” = our typical default for this product type. Edit the buyer column to confirm or change any line.
	Component
	Multistance Standard
	Buyer Specification

	Rash guard main fabric
	88/12 polyester/spandex compression knit
	[  ]

	Rash guard seams
	Flatlock stitching
	[  ]

	Fight shorts main fabric
	4-way stretch woven polyester
	[  ]

	Fight shorts liner
	Compression brief liner
	[  ]

	Waistband
	Elastic + drawcord, grosgrain trim
	[  ]

	Side slits
	Reinforced stretch gusset panel
	[  ]

	Labels
	Woven + printed satin
	[  ]

	Packaging
	Individual polybag
	[  ]


3. Point of Measure (Reference Size)
Values shown are Multistance's standard block at size M. A full graded S–XXL breakdown is available on request.
	Measurement Point
	Multistance Standard
	Buyer Specification

	Rash Guard Chest Width
	52 cm / 20.5"
	[  ]

	Rash Guard Body Length
	68 cm / 26.8"
	[  ]

	Rash Guard Sleeve Length (short)
	22 cm / 8.7"
	[  ]

	Fight Shorts Waist (relaxed, elastic)
	36 cm / 14.2"
	[  ]

	Fight Shorts Hip
	56 cm / 22.0"
	[  ]

	Fight Shorts Inseam
	15 cm / 5.9"
	[  ]


4. Size Reference
Standard US/UK adult unisex block shown for reference — edit or replace with your required size run and labeling convention (numeric UK, EU, custom, etc.).
	Size
	US Unisex
	UK Numeric Chest

	S
	S
	34-36

	M
	M
	38

	L
	L
	40

	XL
	XL
	42

	XXL
	XXL
	44-46


5. Colorway Specification
List each colorway's color name, Pantone code (if known), and hex — final color is confirmed against a physical fabric strike-off, not a screen color.
	Panel / Trim
	Colorway 1
	Colorway 2

	Rash Guard Body
	[  ]
	[  ]

	Rash Guard Sleeve
	[  ]
	[  ]

	Fight Shorts Main
	[  ]
	[  ]

	Fight Shorts Side Panel
	[  ]
	[  ]

	Waistband Trim
	[  ]
	[  ]


6. Construction & Finishing
	Area
	Multistance Standard
	Buyer Preference

	Rash guard seams
	Flatlock stitching throughout
	[  ]

	Fight shorts side slits
	Reinforced 4-way stretch gusset
	[  ]

	Waistband
	Elastic + drawcord, 2 eyelets
	[  ]

	Fabric technology
	Four-way stretch, moisture-wicking
	[  ]


7. Branding & Decoration Placement
	Element
	Multistance Standard Placement
	Buyer Specification

	All-over graphic
	Sublimated front / back / sleeves
	[  ]

	Waistband branding
	Woven or sublimated
	[  ]

	Decoration method
	Sublimation (all-over)
	[  ]


8. Labeling & Packaging
	Item
	Multistance Standard
	Buyer Preference

	Individual packaging
	Recyclable polybag
	[  ]

	Barcode
	EAN/UPC on hangtag
	[  ]

	Carton packing
	By size/color unless specified
	[  ]


9. Additional Notes / Buyer Requirements
Use this space for anything not covered above — reference samples, compliance/testing requirements, special packing instructions, etc.
 
 
 
 
